**Figures captions**

Figure 1. Slag compositions of smelting HCFeMn alloy from other workers’ studies

Figure 2. XRD analysis of HAMO

Figure 2. XRD analysis of HAMO

Figure 4. Specimens appearance of HCFeMn and high-alumina slags (a) in CaO/(SiO2+Al2O3) 0.7 and FC/O 0.9 at 1525℃ for 30 min

Figure 5.Thermodynamics graph of direct reduction (a) and indirect reduction (b) in Mn-Fe ore, the formation of MnxCy (c) and the decompose of MnxCy (d)

Figure 6. Effect of CaO/(SiO2+Al2O3) on the smelting index

Figure 7. Effect of basicity on the liquid slag region of CaO-SiO2-Al2O3-MgO-MnO

Figure 8. XRD patterns of smelting slag with different ternary basicity of CaO/(SiO2+Al2O3)

Figure 9. Effect of smelting FC/O on the smelting separation of HAMO

Figure 10. Thermodynamic equilibrium analyses using FACTSAGE 7.0 with different smelting FC/O values, the Mn, Fe and C mass in metal, and MnO mass in slag

Figure 11. Effect of smelting time on the smelting index

Figure 12. XRD patterns of smelting slag with different smelting time

Figure 13. SEM-EDS analyses of the smelting slag with different smelting time: (A) 15 min, (B) 30 min, (C) 45 min, (D) 60 min and (E) 90 min

Figure 14. Effect of smelting temperature on the smelting index

Figure 15. Morphologies of the separation iron and slag with different smelting temperature

Figure 16. XRD patterns of smelting slag with different smelting temperature

Figure 17. SEM-EDS analysis of the smelting slag with different smelting temperature: (A) 1475℃; (B) 1500℃; (C) 1525℃; (D) 1550℃

Figure 18. SEM-EDS analyses of smelting slag

Figure 19. SEM-EDS analyses of HCFeMn alloy